**HANDHELD SHOWER HOSE SPECIFICATIONS:**

Install a standard length OR two-metre-long handheld shower hose:

* Handheld shower hose to be mounted on: (select one, delete those not applicable and fill in specifications)
* Vertical grabrail – the low end of the grabrail should be 1000mm from the floor of the shower recess and the grabrail should be 1000mm long. (please note that this option can only be done when the stud is located centrally in the shower wall. OT to assess for this before recommending.)
* Hook mountings (stipulate as many mountings as required). E.g. One at 1000mm and one at 1800mm height from the floor of the shower recess.
* Install/retain a fixed shower rose with diverter switch. (Include this if a fixed head shower is to be retained or installed in addition to the HHSH)