**HANDRAIL SPECIFICATIONS:**

Stainless steel OR Galvanised steel OR Aluminium handrail to be installed bilaterally / on left / on right hand side as ascending at the front / rear / other (specify) access:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Height of top edge of handrail** | **Handrail to extend past the bottom riser** | **Handrail attachment point at bottom** | **Handrail to extend horizontally past the top riser** | **Handrail attachment point at top** |
| mm above nose of step | mm | concrete path / ground / pavers / weatherboard / wall of the house | mm | concrete path / ground / pavers / weatherboard / wall of the house |

* Handrails to be constructed and fixed so that there is no obstruction to the passage of the hand along the rail. A 50 mm clear space will exist between the external edge of the handrail and any obstruction. This clearance shall extend above the top of the handrail by not less than 600 mm.
* Cross section of the rails to be circular, and 30– 52 mm external diameter.
* The top 270° of the arc shall be unobstructed for the full length of the handrail.
* Handrails shall be securely fixed and rigid, and their ends shall be turned through a total of 180°, or to the ground, or returned fully to end post or wall face.
* Handrail must be able to withstand force of user who weighs (insert weight) kgs. (Only if over 100kgs).
* if steps greater than 1000mm from ground height to be 1000mm above nose of steps, with vertical balustrades. If a balustrade is required at a height greater than the handrail, both shall be provided.

**PLEASE NOTE**: The recommendations contained in this report are made after consultation with the client/homeowner and an investigation of the client’s circumstances and needs. Their purpose is to outline steps required to be taken for the benefit of the client, with regard to their disability and function. They do not purport to reflect other than limited knowledge on the part of the Occupational Therapist of structural considerations and building codes. **Any queries, concerns or alterations considered necessary for compliance with current building regulations must be discussed with the Occupational Therapist before the work proceeds.**  The Occupational Therapist accepts no responsibility for supervision of the work or the quality of the workmanship.