**THRESHOLD RAMP SPECIFICATIONS:**

Installation of arecycled solid rubber ramp or aluminium ramp atthefront / rear / internal access:

Construct threshold ramp:

|  |  |  |
| --- | --- | --- |
| Height (mm) | Length (mm) | Width (mm) |
|  |  |  |

* From ? to ?.
* Ramp to be installed on carpet OR timber OR tiles OR concrete
* Ramp to have consistent gradient of a maximum gradient to be 1:8.
* Sharp transition at the top and bottom of ramp
* Threshold wedge to be slip resistant, and traversable by wheelchair and walking frame
* Where threshold ramp edges do not abut to wall ramp, shall be tapered or splayed at a minimum of 45°.