**DOORWAY SPECIFICATIONS:**

**Hinged Doorway**

* Remove existing door between room / room and increase doorway opening size to create a **clear** doorway opening of a (insert dimensions) mm. (Minimum of 850 mm as per AS1428.1.)
* Supply and install lever door handles in place of existing door handles.
* Height of handles from finished floor to be (insert dimensions) mm (Between 900 and 1100 mm.)
* Other considerations for OT: Lift off hinges etc

### **Sliding Door**

* Remove existing door between room / room and increase doorway-opening size (on wall that sliding door is attached) to create a **clear** doorway opening of a (insert dimensions) mm. (Minimum of 850 mm.)
* Install new internal cavity / external slider door to fit this doorway opening size.

### **Reswing Door**

* Re-swing door from room / room so that door opens into / out of room, with hinges located on left / right when approaching from bathroom.
* Other considerations for OT: Lift off hinges etc

**Archway**

* Remove existing door between room / room and increase doorway opening size (on catch side of door / on hinged side of door) to create a **clear** doorway opening of a (insert dimensions) mm. (Minimum of 850 mm.)
* Door not to be replaced at this doorway, but instead square archway to be created.

**PLEASE NOTE**: The recommendations contained in this report are made after consultation with the client/homeowner and an investigation of the client’s circumstances and needs. Their purpose is to outline steps required to be taken for the benefit of the client, with regard to their disability and function. They do not purport to reflect other than limited knowledge on the part of the Occupational Therapist of structural considerations and building codes. **Any queries, concerns or alterations considered necessary for compliance with current building regulations must be discussed with the Occupational Therapist before the work proceeds.**  The Occupational Therapist accepts no responsibility for supervision of the work or the quality of the workmanship.